A cartoon of a person and a dog

AI-generated content may be incorrect. Job Safety &

Environmental Analysis

Please return this Document to the Department Lead when complete.

**Company Name:** D. Dastardly Inc **Date:** Department**/Area:** **Inspected By:**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Item | Quantity | Description | Unit Price | Total |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| Team Lead | Forman | Supervisor | Associate |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

|  |  |
| --- | --- |
| Safety Check List | Environmental Check List |
| Management Commitment & Policy  Does the company have a written safety policy?  Is the safety policy communicated to all employees?  Is there a designated safety manager or committee?  Are safety goals and objectives established and reviewed regularly?  Is adequate budget allocated for safety initiatives? | Greenhouse Gas (GHG) Management & Verification  ISO 14064-1:2018 - Greenhouse gases – Part 1: Specification with guidance at the organization level for quantification and reporting of greenhouse gas emissions and removals:  Are organizational GHG emissions (Scope 1, 2, and relevant Scope 3) quantified according to this standard?  Is a GHG inventory report prepared? |

|  |  |  |
| --- | --- | --- |
| PPE Category | PPE Item | Checklist Item/Detail |
| I. Head Protection | Hard Hats (ANSI Z89.1)  Bump Caps | Good condition, proper fit  Minor impact protection |
| II. Eye & Face Protection | Safety Glasses/Goggles (ANSI Z87.1)  Face Shields  Welding Helmets | Clear, intact, appropriate for splash/dust  Full face protection (splashes, debris, heat); secure  Correct shade lens |
| III. Hearing Protection | Earplugs/Earmuffs | Proper fit, good condition |
| IV. Hand Protection | Gloves (hazard-specific) | Correct material, no damage, proper fit |
| V. Body Protection | High-Visibility Clothing (ANSI/ISEA 107)  Aprons/Coveralls  Insulated/Rain Gear | Required class (vests, shirts, jackets)  For chemical, cut, flame, or other specific hazards  For environmental conditions |
| VI. Foot Protection | Safety-Toe Footwear (ASTM F2413)  Metatarsal Guards | Good condition, slip/puncture-resistant soles  Top-of-foot protection |
| VII. Respiratory Protection | Respirators (N95, half/full-mask, supplied-air)  Dust Masks | Fit tested, correct filters, maintained, user trained  For nuisance dust |
| VIII. Fall Protection | Harness, Lanyards, Anchorage (ANSI Z359.11)  Guardrails/Nets | Inspected, no damage, rated points; training  Proper installation and strength |
| IX. Other Specialized PPE | Welding/Arc Flash Protection  Proximity Suits  Impulse Noise Hearing Protection | Appropriate clothing, shields, gloves (NFPA 70E)  For high-heat environments  Specifically rated |